DAMAGES:-
1. Front L/S of the vehicle is badly damaged. L/s Front wheel rim bent & wheel pushed back extensively indicating that the L/S front suspension arms lower; shocker; drive axle; suspension arm upper; support rod are bent/de-aligned. 
2. Bumper front broken. Grills broken; Fog lights broken.
3. Wiring cut/broken.
4. L/S Apron assy; lower supporting members bent & de-aligned. 
5. Bonnet centre dented & deshaped. 
6. Front tie member bent.
7. Radiator & condenser assy. pushed back/bent 
8. Fuse box broken.
9. Air Cleaner broken.
10. L/S front door dented at front edge
11. Battery excide pressed.
12. Left side lower running board dented.
13. Oil sump dented. 
14. Exhaust manifold & pipe dented. 
15. Dash board cracked/broken.
16. Right side apron dented/bent at centre point.
17. Left side rear door & L/S Qtr. Panel dented. 
18. Tail Light L/S broken.
19. Rear Bumper broken at L/S
20. R/S Fender dented/Twisted as there is gap between the door & fender.
21. Both head lights broken.
22. Steering system damaged; L/S tie rod bent.
23. Engine foundations broken.
24. The above are the externally visible damages & any other damage noted during repairs shall be taken into account, keeping in view the nature/cause of the accident.  



