FOLLOWING DAMAGES ARE NOTED:-

1. Cabin:- Cabin of the vehicle is totally damaged, the wooden pcs. are scattered on the hill surface.

2. Cowl Assy:- Cowl assy. of the vehicle is badly damaged. Front W/S glass frames, lower supporting members; Floor side bonnet assy; Bonnet centre; Dash board etc are damaged in such a way that the cowl assy. is not economically/satisfactory repairable. 

3. Chassis Frame:- Chassis Frame bent at multiple points. Engine founds; Gear box foundations broken.

4. Main Tank:- All sides of the main tank dented & deshaped, side de-canting pipes dented/bent. Upper platform bent/twisted. U. Bolts broken; rubber pads broken.

5. Pipes:- All diesel, brake, Air pipes broken/bent/twisted.

6. Battery:- Battery broken – battery cables broken.
7. Electrical Wiring:- Complete wiring broken.

8. Brake:- Brake booster, air tanks broken/dented.

9. Front Suspension:- Front Spring leaves assy. intact with chassis frame; tie rods; drag links; tie rod ends broken, steering arms bent; front axle, tie rod de-aligned

10. Rear Suspension:- Rear Suspension (Rear Differential tube) may be de-aligned; U/C Bolts broken; Spring leaves assy. broken.

11. Propeller Shaft:- Both front/rear propeller shafts bent; c-bearing broken; male-female unit of rear propeller shaft broken.

12. Engine Assy:- Oil Sump (Chamber) dented; water body broken; water pipes dented; alternator broken, self starter broken. Both the items are fixed with the engine assy. clutch assy. broken main shaft of gear box broken. However gear box externally ok.

13. Radiator assy:- Radiator assy. badly damaged. Fan broken.

14. Steering:- Steering wheel broken. Steering column U/J cross, steering rod bent/de-aligned. Steering box OK.
  
