DAMAGES:-

1. Body Shell:- L/S of the body shell is totally dented/damaged; roof dented & buldged; L/S Front door; centre pillar; Front W/S glass frame; Front Pillar; Centre Pillar; Qtr. Panel L/S; Front Fender; Bonnet centre; Dicky panel; R/S Qtr. Panel; Right side Front door; R/S front fender dented & deshaped; Rear View mirror both sides broken. Dash panel/cowl top panel dented/bent; Dicky dented/bent. The body shell of the vehicle is allowed.
2. L/S Apron badly bent/twisted & welding uprooted.
3. Internal Dash Board/Instrumental panel broken. Steering wheel bent.
4. Front W/S glass broken; L/S Front door glass broken.
5. Front & Rear Bumper bent/pressed/de-framed. 
6. Inner upholstery bent/twisted.
7. Radiator & Condenser Assy. bent.
8. Front Grills broken.
9. Wiper arms/blade bent.
10. Front head light broken.
11. L/S Front Wheel bent – de-aligned.
12. Wiring seems cut. 

