DAMAGES:-

1. Load body (Scoop) has separated from chassis frame which is lying on the slope of the hill. The back side dalla and front portion which is generally on cabin roof are badly bent. The both sides sheets are also bent/de-aligned.
2. Sub-Frame assy. bent.
3. Chassis frame extensively bent beyond repairs.
4. Radiator; Inter-cooler & fan assy. damaged. 
5. Cabin along with front windshield glass, upholstery, dash board, meter panel & all other fittings totally smashed and damaged. It’s roof uprooted & lying at different places. 
6. Most of wheel rims are bent and externally tyres are torn.
7. Diesel Tank broken and diesel pipes are bent.
8. Air pipes, pressure pipes are broken/bent.
9. Battery broken.
10. Air tanks dented. 
11. Rear Suspension assy. (Differential tube Assy.) hanger & shackle assemblies of Spring leafs broken & spring leaves lying on ground. U & C Bolts bent. It seems that the rear differential assy. have an impact on it which needs to be checked after recovery.
12. Front Suspension assy. got separated from chassis frame & lying at a distance of approx.. 50 feet from the vehicle; Front axle, tie rods & Links are bent & de-aligned. 
13. Gear box assy. & engine assy. got broken from chassis after breaking the engine foundation & lying about 10 feet (Approx.) from the vehicle
14. Brake chambers fixed with front axle & rear axle (4 no. in all) pressed & damaged. 
15. Complete wiring either cut/broken.
16. The engine assy. was partially submerged in pebbles/mud. It seems the engine fuel pump & other components are damaged.   

The above are the externally visible damages and there is every possibility that some other damages may came to light when the vehicle is dismantled for repairs, which shall be taken into a/c keeping in view the Nature of loss.   

Lateron, it was discussed with the insured to retrieve the vehicle from the site of accident and to keep the same in safe custody. The insured brought the vehicle to Jatwal which is about 40 Kms. from Jammu on Jammu – Pathankot Road. I along with worth Sr. Branch Manager visited the place and checked the vehicle. Following other damages were seen.

1. Engine assy:- The tapet cover of the vehicle is broken & separated mud/sand has entered the cylinder head parts, resulting in internal damages to the engine assy. & oil sump dented & sheet torn. Engine pulley broken; timing side of the engine assy. damaged.
2. Propeller shafts bent, their male/female units broken.
     Gear Box housing broken/cracked.
