EXTERNALLY VISIBLE DAMAGES:-

1. Bonnet Assy. L/S portion dented.
2. L/S Fender & Apron assy. bent/dented.
3. L/S Tyre Shifted backwardly.
4. Cross-member & Lower member bent.
5. Left side front suspension assy. i.e, arms, shocker, knuckle hub; wheel rim etc. bent/damaged.
6. Condenser & Radiator assy. bent.
7. All Pipes broken.
8. Rear View mirror broken.
9. L/S Rear Tyre broken; Wheel Rim bent.
10. Rear Axle tube bent.
11. Shocker bent.
12. Drive Axle broken.
13. Suspension Arm bent.
14. Head Lights broken.
15. Bumper Front & Grills broken.
16. Rear Bumper broken.
17. Front Tie member broken/bent.
18. L/s Rear door dented.
19. L/S Rear Qtr. Panel dented.
20. Diesel Tank Pipe Lid broken.
21. Qtr. Panel L/S dented.
22. Tail Light cracked. 
23. Dicky Panel bent.
24. Bumper Support panel bent.
25. Wiring cut/broken.

