DAMAGES
1. Right side fender and centre bonnet dented & deshaped.
2. Right side & Left side head lights broken.

3. Front Bumper broken and its inner parts bent.

4. Front W/S glass broken.

5. Wheel Rim bent & tyre cut/torn.

6. Apron Assy. bent/dented/twisted/deshaped.
7. PCM bent/twisted.

8. Battery broken, casing cracked.

9. L/S Front door damaged needs replacement.

10. L/S Rear view mirror broken.

11. Body R/S inner panel bent/twisted.

12. L/S Front tyre shifted towards back side as such the lower suspension arm and inner parts may be damaged, which can be checked only on opening the vehicle.

13. Wiring cut.

14. R/S Fender dented.

15. Front upper member broken.

16. L/S Front door glass broken; weather strips bent, glass regulating machine bent.

17. Cowl top dented/bent.

18. Dash panel shifted backwardly.

19. Dash board cracked.

20. Radiator, condenser assy. needs check on opening the damaged parts, but seems bent/shifted backwardly.

21. Cross-member de-aligned, spindle shocker bent de-aligned. 

The above are the externally visible damages and there is every possibility that some other damages may came to fore-front when the vehicle is dismantled for repairs. 

.

