DAMAGES:-


1.	Body Shell:- The Front both aprons of the vehicle are badly damaged. Front member bent, both side fenders dented. R/S Apron totally damaged. L/S Apron uprooted at the cowl top joint. Dash panel bent, Cowl panel dented/bent, roof damaged. Both side body panels dented. Right side both doors dented, L/S door out of alignment. Front W/S Glass broken. Both side vertical members bent/twisted. Whole of the body shell damaged and beyond satisfactory repairs, for which reason cost of new body shell is recommended.
2.	Radiator/Condenser Assy. damaged.
3.	Shrouds broken.
4.	Bonnet Assy. dented.
5.	Front tie member bent.
6.	Front Bumper, head light, parking, Fog lights broken.
7.	Instrumental panel broken.
8.	Steering wheel bent.
9.	Wiring cut/broken.

