DAMAGES:-

1.	Bonnet Centre; L/S Fender; R/S Fender; cowl panel; glass panel; L/S body panel; L/s door, roof; rear dicky. L/S Body panel; Front tie member; R/S Fender; L/S Rear door are badly dented/damaged. The body shell is damaged in such a way that it is not repairable and its replacement is necessitated.
2.	Front W/S Glass broken; rear dicky panel glass; L/S front door glass; rear mirror glass broken. 
3.	Dash board broken.
4.	Tail Light broken.
5.	Radiator & Condenser assy. bent/twisted. 
6.	Engine cover broken.
7.	Fuel injection pump broken.
8.	L/S Apron assy. dented.
9.	L/S shocker upper, nut/bolt joints broken.
10.	Air Cleaner broken.
11.	Wiper arms/blade; linkages bent/twisted.
12.	A.C. Pipes broken/pressed.
13.	Cylinder head damaged.
14.	HVAC unit broken.
15.	Steering wheel bent & it seems that steering column is also bent.

