DAMAGES:-


1.	Load Body/Cabin:- Totally damaged – Not repairable. 
2.	Cowl Assy.:- Show/Cowl assy. totally damaged/dented/deshaped.
3.	Chassis Frame:- Badly bent/twisted. It cannot be repaired.
4.	Engine Assy.:- The Engine assy. is damaged; alternator damaged; self damaged & engine foundations broken.
5.	Front Suspension:- Front Suspension of the vehicle got separated from the chassis frame. Shackle/Hanger assys. broken; U/C Bolts bent; Spring leaves assys. distorted/bent/broken; tie rod long; small; link rods bent; tie rod ends broken; brake pipes bent.
6.	Rear Suspension:- Rear Suspension assy. broken from the chassis frame. Hanger/Shackle assy. broken; U/C Bolts bent; Spring leaves assy. distorted/bent. 
7.	Electrical System:- Meter panels along with Meters broken; wiring completely broken; Switch broken.
8.	Brake System:- Brake System totally damaged.
9.	Battery:- broken.
10.	Diesel Tank:- Dented/deshaped – Diesel Pipes bent.


